**Clay Hardness Statement**

Customers are advised that our standard clay hardness using a clay hardness penetrometer (pig-stick) is 6.0 – 7.5, this is due to the nature of the production process. During storage the penetrometer value may then increase.

Specific clay hardness requirements which fall outside the standard range need to be requested at the point of ordering.